IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-08-22T16:18:46"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150220_1215(x64) - Exporter 16.0.428.0 - Default UI"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "ksubramanya" of Organization (no name given)
  Owner history of Person "ksubramanya" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 2 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "std" | object type "std" | names: "ZZZ_do not use_ME_ST_UN_lipator s options_ACO:std:305114" | material: materials ("PVC, White", "HDPE, Red", "Stainless Steel, Grade 316", "Plastic, Clear") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, General, Identity Data
          1 x IFCENERGYCONVERSIONDEVICE | type IFCCOILTYPE "std" | object type "std" | names: "ZZZ_do not use_ME_ST_WPB_heating rod_ACO:std:305134" | material: materials ("Copper", "HDPE, Black") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Loads, Electrical Engineering

Types
  IFCBUILDINGELEMENTPROXYTYPE "std" | USERDEFINED | 1 occurrence | material: materials ("PVC, White", "HDPE, Red", "Stainless Steel, Grade 316", "Plastic, Clear") | property sets: Identity Data, Other
  IFCCOILTYPE "std" | USERDEFINED | 1 occurrence | material: materials ("Copper", "HDPE, Black") | property sets: Constraints, Electrical - Loads, Electrical Engineering, General, Identity Data, Materials and Finishes | description "ACO heating rod"

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "ZZZ_do not use_ME_ST_UN_lipator s options_ACO: std" (IFCLABEL)
    Family and Type = "ZZZ_do not use_ME_ST_UN_lipator s options_ACO: std" (IFCLABEL)
    L2_half = 485. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    R1 = 318.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "ZZZ_do not use_ME_ST_UN_lipator s options_ACO: std" (IFCLABEL)
    Type Id = "ZZZ_do not use_ME_ST_UN_lipator s options_ACO: std" (IFCLABEL)
    blend_position = 327. (IFCLENGTHMEASURE) [MILLI METRE]
    bottom_extension_type2 = TRUE (IFCBOOLEAN)
    conevent_out_L1_calculated = 145. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_out_L2_calculated = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_out_angle2_calculated = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    disabled_options = FALSE (IFCBOOLEAN)
    flanged_sludge_connection = FALSE (IFCBOOLEAN)
    footing_type1 = FALSE (IFCBOOLEAN)
    footing_type2 = TRUE (IFCBOOLEAN)
    grease_connection_type2 = TRUE (IFCBOOLEAN)
    grease_pipe_length_calculated = 312.2 (IFCLENGTHMEASURE) [MILLI METRE]
    greasevent_in_L1_calculated = 127. (IFCLENGTHMEASURE) [MILLI METRE]
    greasevent_in_L2_calculated = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    greasevent_in_angle3_calculated = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    heatrod_option = 0 (IFCINTEGER)
    inlet_angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    lookup_table_name = "lipator_s" (IFCTEXT)
    motor_valve_toggle = FALSE (IFCBOOLEAN)
    non_flanged_sludge_connection = TRUE (IFCBOOLEAN)
    options_lookup_table_name = "lipator_s_options" (IFCTEXT)
    outlet_angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev10_end = -40. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev10_start = -45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev11_end = 155. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev11_start = 150. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev12_end = -40. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev12_start = -45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev13_end = 35. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev13_start = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev14_end = 50. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev14_start = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev15_end = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev15_start = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev1_end = 95. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev1_start = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev2_end = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev2_start = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev3_end = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev3_start = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev4_end = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev4_start = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev5_end = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev5_start = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev6_end = 117. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev6_start = 112. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev7_end = 275. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev7_start = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev8_end = 95. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev8_start = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev9_end = 230. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rev9_start = 225. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    sludge_X3_calculated = 311.834090503267 (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_Z2_calculated = 468. (IFCLENGTHMEASURE) [MILLI METRE]
    sludgevent_in_L1_calculated = 127. (IFCLENGTHMEASURE) [MILLI METRE]
    sludgevent_in_L2_calculated = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    sludgevent_in_angle3_calculated = -90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    switchbox_toggle = TRUE (IFCBOOLEAN)
    type_index = 2 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "ZZZ_do not use_ME_ST_WPB_heating rod_ACO: std" (IFCLABEL)
    Family and Type = "ZZZ_do not use_ME_ST_WPB_heating rod_ACO: std" (IFCLABEL)
    Type = "ZZZ_do not use_ME_ST_WPB_heating rod_ACO: std" (IFCLABEL)
    Type Id = "ZZZ_do not use_ME_ST_WPB_heating rod_ACO: std" (IFCLABEL)
    help_connected_phase = 3 (IFCINTEGER)
    option = 0 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Circle Head - Project Datum" (IFCLABEL)
    Family and Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type Id = "Level: Circle Head - Project Datum" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "ZZZ_do not use_ME_ST_UN_lipator s options_ACO" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "ZZZ_do not use_ME_ST_WPB_heating rod_ACO" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Circle Head - Project Datum" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "3" (IFCTEXT)
    RSen_C_code_article = "7300.01.00" (IFCTEXT)
    RSen_C_code_gtin = "04002626340702" (IFCTEXT)
    RSen_C_description = "ACO Heizpatrone mit Steuerung" (IFCTEXT)
    RSen_C_product_assortment = "Grease separators" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 0" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Manufacturer = "ACO" (IFCTEXT)
    Model = "" (IFCTEXT)
    OmniClass Number = "23.70.50.00" (IFCTEXT)
    OmniClass Title = "Liquid Waste Handling Services" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "std" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "ACO heating rod" (IFCTEXT)
    LOD = "LOD 400" (IFCTEXT)
    Manufacturer = "ACO" (IFCTEXT)
    Model = "Heating rod" (IFCTEXT)
    OmniClass Number = "23.70.50.00" (IFCTEXT)
    OmniClass Title = "Liquid Waste Handling Services" (IFCTEXT)
    Type Comments = "kpl., 6.0kW, 3x400V" (IFCTEXT)
    Type Name = "std" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Anno_Level_Head_Circle: Standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = FALSE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "std" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "ACO" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 0" (IFCTEXT)
    Level = "Level: Level 0" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    grease_angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    grease_connection_angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    heating_rod = TRUE (IFCBOOLEAN)
    sludge_connection_angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 0" (IFCTEXT)
    Level = "Level: Level 0" (IFCLABEL)
    Offset = 1396.11700561653 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 4.12968522164257 (IFCAREAMEASURE) [SQUARE_METRE]
    D = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    D1 = 637. (IFCLENGTHMEASURE) [MILLI METRE]
    D2 = 504. (IFCLENGTHMEASURE) [MILLI METRE]
    D3 = 504. (IFCLENGTHMEASURE) [MILLI METRE]
    D4 = 450. (IFCLENGTHMEASURE) [MILLI METRE]
    D5 = 114.3 (IFCLENGTHMEASURE) [MILLI METRE]
    DN = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Do2_outlet = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Do2_sludge = 220. (IFCLENGTHMEASURE) [MILLI METRE]
    Do3_sludge = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Do_bottom_extension = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Do_bottom_flange = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Do_bypass = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Do_conevent_in = 26.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Do_conevent_out = 26.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Do_grease = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Do_greasevent_in = 26.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Do_inlet = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Do_outlet = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Do_sludge = 114.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Do_sludgevent_in = 26.9 (IFCLENGTHMEASURE) [MILLI METRE]
    H = 1700. (IFCLENGTHMEASURE) [MILLI METRE]
    H1 = 1300. (IFCLENGTHMEASURE) [MILLI METRE]
    H11 = 822. (IFCLENGTHMEASURE) [MILLI METRE]
    H12 = 852. (IFCLENGTHMEASURE) [MILLI METRE]
    H13 = 862. (IFCLENGTHMEASURE) [MILLI METRE]
    H14 = 990. (IFCLENGTHMEASURE) [MILLI METRE]
    H15 = 1487. (IFCLENGTHMEASURE) [MILLI METRE]
    H2 = 1230. (IFCLENGTHMEASURE) [MILLI METRE]
    H21 = 1707. (IFCLENGTHMEASURE) [MILLI METRE]
    H22 = 415. (IFCLENGTHMEASURE) [MILLI METRE]
    H23 = 1569. (IFCLENGTHMEASURE) [MILLI METRE]
    H24 = 415. (IFCLENGTHMEASURE) [MILLI METRE]
    H25 = 1069. (IFCLENGTHMEASURE) [MILLI METRE]
    H26 = 1395. (IFCLENGTHMEASURE) [MILLI METRE]
    L1 = 640. (IFCLENGTHMEASURE) [MILLI METRE]
    L11 = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    L12 = 259.4 (IFCLENGTHMEASURE) [MILLI METRE]
    L13 = 448. (IFCLENGTHMEASURE) [MILLI METRE]
    L2 = 970. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.318372233202932 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    bottom_diam = 115.4 (IFCLENGTHMEASURE) [MILLI METRE]
    bottom_extension_H = 78. (IFCLENGTHMEASURE) [MILLI METRE]
    bottom_flange_H = 18. (IFCLENGTHMEASURE) [MILLI METRE]
    bottom_length = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    bottom_offset = 127. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_in_L = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_in_X = 552. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_in_Y = 913. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_in_Z = 1569. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_in_angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    conevent_in_angle2 = 225. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    conevent_out_L = 190. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_out_L2 = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_out_X = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_out_Y = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_out_Z = 1460. (IFCLENGTHMEASURE) [MILLI METRE]
    conevent_out_angle = -45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    footing_height = 494. (IFCLENGTHMEASURE) [MILLI METRE]
    footing_height2 = 382. (IFCLENGTHMEASURE) [MILLI METRE]
    footing_radius = 375. (IFCLENGTHMEASURE) [MILLI METRE]
    grease_H = 1040. (IFCLENGTHMEASURE) [MILLI METRE]
    grease_X = 379.2 (IFCLENGTHMEASURE) [MILLI METRE]
    grease_valve_X = 236.6 (IFCLENGTHMEASURE) [MILLI METRE]
    grease_valve_angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    greasevent_in_L = 172. (IFCLENGTHMEASURE) [MILLI METRE]
    greasevent_in_L2 = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    greasevent_in_X = 552. (IFCLENGTHMEASURE) [MILLI METRE]
    greasevent_in_Y = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    greasevent_in_Z = 1569. (IFCLENGTHMEASURE) [MILLI METRE]
    greasevent_in_angle = -60. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    greasevent_in_angle2 = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    inlet_X = 552. (IFCLENGTHMEASURE) [MILLI METRE]
    inlet_Y = 740.6 (IFCLENGTHMEASURE) [MILLI METRE]
    inlet_length = 157. (IFCLENGTHMEASURE) [MILLI METRE]
    leg_offset = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    legnumber = 4 (IFCINTEGER)
    outlet_X = 552. (IFCLENGTHMEASURE) [MILLI METRE]
    outlet_X2 = 552. (IFCLENGTHMEASURE) [MILLI METRE]
    outlet_Y = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    outlet_length = 157. (IFCLENGTHMEASURE) [MILLI METRE]
    rib1_Z = 872. (IFCLENGTHMEASURE) [MILLI METRE]
    rib1_diameter = 534.1 (IFCLENGTHMEASURE) [MILLI METRE]
    rib2_Z = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    rib2_diameter = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    rib_number = 1 (IFCINTEGER)
    rib_thickness = 35. (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_H = 884. (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_L1 = 418.2 (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_X = 418.2 (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_X2 = 220.5 (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_Z = 74. (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_angle = 112. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    sludge_flange_L = 23.5 (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_flange_position = 398.2 (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_valve_Z = 407.5 (IFCLENGTHMEASURE) [MILLI METRE]
    sludge_valve_angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    sludgevent_in_L = 172. (IFCLENGTHMEASURE) [MILLI METRE]
    sludgevent_in_L2 = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    sludgevent_in_X = 552. (IFCLENGTHMEASURE) [MILLI METRE]
    sludgevent_in_Y = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    sludgevent_in_Z = 1569. (IFCLENGTHMEASURE) [MILLI METRE]
    sludgevent_in_angle = 60. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    sludgevent_in_angle2 = -45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Area = 0.0525643619160268 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00124856280926294 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    RSen_P_c01_diameter = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_diameter = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 type object
    RSen_C_code_ETIM = "EC001118" (IFCTEXT)
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_code_specification_URL = "" (IFCTEXT)
    RSen_C_content_creator = "Itannex bv" (IFCTEXT)
    RSen_C_content_date_changed = "" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "" (IFCTEXT)
    RSen_C_info_technical = "" (IFCTEXT)
    RSen_C_intended_use = "Entwässerungssysteme" (IFCTEXT)
    installation_manual = "" (IFCTEXT)
    instructions_for_use = "" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    RSen_C_material = "Stainless Steel, Grade 316" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "HDPE, Black" (IFCLABEL)
  Model Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    heatrod_X = 318.5 (IFCLENGTHMEASURE) [MILLI METRE]
    heatrod_Z = 747. (IFCLENGTHMEASURE) [MILLI METRE]
    heatrod_angle = 150. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    heatrod_angle2 = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    switchbox_X = 944.85 (IFCLENGTHMEASURE) [MILLI METRE]
    switchbox_Y = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    switchbox_Z = 1316.5 (IFCLENGTHMEASURE) [MILLI METRE]
    switchbox_angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Phasing | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Reference = "std" (IFCIDENTIFIER)
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
    RSen_E_c01_apparent_power_phase_1 = 2000. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_2 = 2000. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_3 = 2000. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 1 type object
    RSen_E_c01_load_classification = "Power" (IFCLABEL)
    RSen_E_powerfactor = 1. (IFCREAL)
  Electrical Engineering | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_E_c01_apparent_power = 6000. (IFCPOWERMEASURE) [WATT]
    RSen_E_connected_fase = 1 (IFCINTEGER)
  Electrical Engineering | properties | on 1 type object
    RSen_E_c01_3_phase = TRUE (IFCBOOLEAN)
    RSen_E_c01_current = 15. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c01_number_of_poles = 3 (IFCINTEGER)
    RSen_E_c01_subclass_motor = FALSE (IFCBOOLEAN)
    RSen_E_c01_voltage = 400. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    System Classification = "Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Structural | properties | on 1 type object
    RSen_S_net_mass = 15. (IFCREAL)