IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView, QuantityTakeOffAddOnView]"
Time stamp: "2017-05-23T10:17:09"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Default UI"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "palleri" of Organization (no name given)
  Owner history of Person "palleri" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1495514806 (2017-05-23T04:46:46Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCFLOWTERMINAL | type IFCWASTETERMINALTYPE "std" | object type "std" | names: "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO:std:13297" | material: materials ("HDPE, Grey", "HDPE, Red") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Model Properties
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "std" | object type "std" | names: "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO:std:13307" | material: "Stainless Steel, Brushed" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Other

Types
  IFCWASTETERMINALTYPE "std" | GREASEINTERCEPTOR | 1 occurrence | material: materials ("HDPE, Grey", "HDPE, Red") | property sets: Identity Data, Materials and Finishes, Other
  IFCVALVETYPE "std" | FAUCET | 1 occurrence | material: "Stainless Steel, Brushed" | property sets: Constraints, General, Identity Data, Materials and Finishes, Other, Plumbing | description "Filling device"

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    B_half = 475. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    F_arc_Z_centre_pos = 135. (IFCLENGTHMEASURE) [MILLI METRE]
    Family = "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO: std" (IFCLABEL)
    Family and Type = "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO: std" (IFCLABEL)
    L2_half = 1242.5 (IFCLENGTHMEASURE) [MILLI METRE]
    LF_half = 1125. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO: std" (IFCLABEL)
    Type Id = "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO: std" (IFCLABEL)
    access_exit_visibility = TRUE (IFCBOOLEAN)
    body_height = 1463. (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_option = 1 (IFCINTEGER)
    grease_measure_option = 1 (IFCINTEGER)
    heatrod_option = 1 (IFCINTEGER)
    lookup_table_name = "eco-jet_o_basic_type" (IFCTEXT)
    options_lookup_table_name = "eco-jet_options" (IFCTEXT)
    sight_glas_option = 1 (IFCINTEGER)
    type_index = 85 (IFCINTEGER)
    vent_at_entry_check = FALSE (IFCBOOLEAN)
    vent_connector_length = 1160. (IFCLENGTHMEASURE) [MILLI METRE]
    vent_connector_position = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO: std" (IFCLABEL)
    Family and Type = "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO: std" (IFCLABEL)
    Type = "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO: std" (IFCLABEL)
    Type Id = "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO: std" (IFCLABEL)
    option = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "20" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "21" (IFCTEXT)
    RSen_C_code_article = "3300.11.22" (IFCTEXT)
    RSen_C_code_gtin = "04002626299253" (IFCTEXT)
    RSen_C_description = "ACO Fülleinheit für Eco-Jet-O,-OD,-R,-RD" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Manufacturer = "ACO" (IFCTEXT)
    Model = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "std" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Filling device" (IFCTEXT)
    LOD = "LOD 400" (IFCTEXT)
    Manufacturer = "ACO" (IFCTEXT)
    Model = "ACO filling device for Ecojet" (IFCTEXT)
    OmniClass Number = "23.70.50.00" (IFCTEXT)
    OmniClass Title = "Liquid Waste Handling Services" (IFCTEXT)
    Type Comments = "Free outlet as per DIN 1988 Part 4" (IFCTEXT)
    Type Name = "std" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (1 IFCFLOWCONTROLLER, 1 IFCFLOWTERMINAL)
    Manufacturer = "ACO" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (1 IFCFLOWCONTROLLER, 1 IFCFLOWTERMINAL)
    Reference = "std" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device = TRUE (IFCBOOLEAN)
    grease_measure_device = FALSE (IFCBOOLEAN)
    heating_rod = FALSE (IFCBOOLEAN)
    inlet_angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    left = TRUE (IFCBOOLEAN)
    right = FALSE (IFCBOOLEAN)
    sight_glass = FALSE (IFCBOOLEAN)
    vent_at_entry = FALSE (IFCBOOLEAN)
    vent_at_exit = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1472.6 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 type object
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 21.8911061232118 (IFCAREAMEASURE) [SQUARE_METRE]
    B = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    D = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    DN = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    DN_vent = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    D_vent = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    FH = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    FW = 230. (IFCLENGTHMEASURE) [MILLI METRE]
    H1 = 1250. (IFCLENGTHMEASURE) [MILLI METRE]
    H2 = 1180. (IFCLENGTHMEASURE) [MILLI METRE]
    H3 = 1880. (IFCLENGTHMEASURE) [MILLI METRE]
    H4 = 1700. (IFCLENGTHMEASURE) [MILLI METRE]
    L1 = 2250. (IFCLENGTHMEASURE) [MILLI METRE]
    L2 = 2485. (IFCLENGTHMEASURE) [MILLI METRE]
    LF = 2250. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 3.93701149525586 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    W1 = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    W2 = 1020. (IFCLENGTHMEASURE) [MILLI METRE]
    access_entry = 1 (IFCINTEGER)
    access_entry_X_position = 280. (IFCLENGTHMEASURE) [MILLI METRE]
    access_entry_diameter = 470. (IFCLENGTHMEASURE) [MILLI METRE]
    access_exit = 1 (IFCINTEGER)
    cover_Z_position = 1587. (IFCLENGTHMEASURE) [MILLI METRE]
    rib_height = 1563. (IFCLENGTHMEASURE) [MILLI METRE]
    rib_number = 7 (IFCINTEGER)
    rib_width = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    vent_Z_position = 1522. (IFCLENGTHMEASURE) [MILLI METRE]
    vent_length = 315. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.076167150313411 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00141803315444823 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Model Properties | properties | on 1 object (1 IFCFLOWTERMINAL)
    filling_device_CL = 272.6 (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_X = 1765. (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_Y = 666. (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_Z = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_position = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    glass_X = 1852.5 (IFCLENGTHMEASURE) [MILLI METRE]
    glass_Z = 1130.5 (IFCLENGTHMEASURE) [MILLI METRE]
    glass_position = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    grease_measure_X = 530. (IFCLENGTHMEASURE) [MILLI METRE]
    grease_measure_Y = 175. (IFCLENGTHMEASURE) [MILLI METRE]
    grease_measure_Z = 1563. (IFCLENGTHMEASURE) [MILLI METRE]
    grease_measure_end_angle = 85. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    grease_measure_position = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    grease_measure_start_angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    heatrod_X = 1540. (IFCLENGTHMEASURE) [MILLI METRE]
    heatrod_Z = 912. (IFCLENGTHMEASURE) [MILLI METRE]
    heatrod_position = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    waterinlet_end_angle = -40. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    waterinlet_start_angle = -45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Phasing | properties | on 2 objects (1 IFCFLOWCONTROLLER, 1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "HDPE, Grey" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "Stainless Steel, Brushed" (IFCLABEL)
  General | properties | on 1 type object
    RSen_C_code_ETIM = "EC010071" (IFCTEXT)
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_code_specification_URL = "" (IFCTEXT)
    RSen_C_content_creator = "Itannex bv" (IFCTEXT)
    RSen_C_content_date_changed = "" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "" (IFCTEXT)
    RSen_C_info_technical = "" (IFCTEXT)
    RSen_P_c01_diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    installation_manual = "" (IFCTEXT)
    instructions_for_use = "" (IFCTEXT)
  Plumbing | properties | on 1 type object
    p_c01_flow = 0.105944000164466 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Structural | properties | on 1 type object
    RSen_S_net_mass = 3.5 (IFCREAL)