IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-08-09T14:20:10"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150220_1215(x64) - Exporter 16.0.428.0 - Default UI"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "ksubramanya" of Organization (no name given)
  Owner history of Person "ksubramanya" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 4 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "NS3" | object type "NS3" | names: "ME_PE_lipusmart p ob_ACO:NS3:306752" | material: materials ("Steel, Blue", "Stainless Steel, Brushed", "HDPE, Grey", "HDPE, Red") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical - Loads, Electrical Engineering
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "std" | object type "std" | names: "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO:std:306753" | material: materials ("HDPE, Grey", "HDPE, Red") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Model Properties
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "std" | object type "std" | names: "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO:std:306756" | material: "Stainless Steel, Brushed" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Other
          1 x IFCDISTRIBUTIONCONTROLELEMENT | type IFCSENSORTYPE "std" | object type "std" | names: "ZZZ_do not use_ME_ST_measuring device for grease_ACO:std:306757" | material: materials ("PVC, Grey", "HDPE, Black", "PVC, White", "Stainless Steel, Brushed") | property sets: Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical - Loads, Electrical Engineering, General

Types
  IFCBUILDINGELEMENTPROXYTYPE "NS3" | USERDEFINED | 1 occurrence | material: materials ("Steel, Blue", "Stainless Steel, Brushed", "HDPE, Grey", "HDPE, Red") | property sets: Electrical - Loads, Electrical Engineering, General, Identity Data, Materials and Finishes, Other | description "Grease separator plant as per DIN EN 1825 and DIN 4040-100"
  IFCBUILDINGELEMENTPROXYTYPE "std" | USERDEFINED | 1 occurrence | material: materials ("HDPE, Grey", "HDPE, Red") | property sets: Identity Data, Materials and Finishes, Other
  IFCVALVETYPE "std" | FAUCET | 1 occurrence | material: "Stainless Steel, Brushed" | property sets: Constraints, General, Identity Data, Materials and Finishes, Other, Plumbing | description "Filling device"
  IFCSENSORTYPE "std" | CO2SENSOR | 1 occurrence | material: materials ("PVC, Grey", "HDPE, Black", "PVC, White", "Stainless Steel, Brushed") | property sets: Constraints, Electrical - Loads, Electrical Engineering, General, Identity Data, Materials and Finishes | description "Measuring device for grease layers"

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    B_half = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "ME_PE_lipusmart p ob_ACO: NS3" (IFCLABEL)
    Family and Type = "ME_PE_lipusmart p ob_ACO: NS3" (IFCLABEL)
    L2_half = 825. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "ME_PE_lipusmart p ob_ACO: NS3" (IFCLABEL)
    Type Id = "ME_PE_lipusmart p ob_ACO: NS3" (IFCLABEL)
    cold_water_connector = "cw in" (IFCTEXT)
    connector_escape_message = "Nicht verwenden" (IFCTEXT)
    help_connected_phase = 3 (IFCINTEGER)
    lipusmart_lookup_table_name = "lipusmart" (IFCTEXT)
    lipusmart_type = 1 (IFCINTEGER)
    lookup_table_name = "eco-jet_o_basic_type" (IFCTEXT)
    no_option = 0 (IFCINTEGER)
    option = 1 (IFCINTEGER)
    options_lookup_table_name = "eco-jet_options" (IFCTEXT)
    vent_at_entry_check = TRUE (IFCBOOLEAN)
    vent_connector_length = 740. (IFCLENGTHMEASURE) [MILLI METRE]
    vent_connector_position = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    B_half = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    F_arc_Z_centre_pos = 135. (IFCLENGTHMEASURE) [MILLI METRE]
    Family = "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO: std" (IFCLABEL)
    Family and Type = "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO: std" (IFCLABEL)
    L2_half = 825. (IFCLENGTHMEASURE) [MILLI METRE]
    LF_half = 705. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO: std" (IFCLABEL)
    Type Id = "ZZZ_do not use_ME_PE_eco-jet_o_options_ACO: std" (IFCLABEL)
    access_exit_visibility = TRUE (IFCBOOLEAN)
    body_height = 1252. (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_option = 1 (IFCINTEGER)
    grease_measure_option = 1 (IFCINTEGER)
    heatrod_option = 1 (IFCINTEGER)
    lookup_table_name = "eco-jet_o_basic_type" (IFCTEXT)
    options_lookup_table_name = "eco-jet_options" (IFCTEXT)
    sight_glas_option = 1 (IFCINTEGER)
    type_index = 3 (IFCINTEGER)
    vent_at_entry_check = FALSE (IFCBOOLEAN)
    vent_connector_length = 740. (IFCLENGTHMEASURE) [MILLI METRE]
    vent_connector_position = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO: std" (IFCLABEL)
    Family and Type = "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO: std" (IFCLABEL)
    Type = "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO: std" (IFCLABEL)
    Type Id = "ZZZ_do not use_ME_ST_filling device for Ecojet_ACO: std" (IFCLABEL)
    option = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "ZZZ_do not use_ME_ST_measuring device for grease_ACO: std" (IFCLABEL)
    Family and Type = "ZZZ_do not use_ME_ST_measuring device for grease_ACO: std" (IFCLABEL)
    Type = "ZZZ_do not use_ME_ST_measuring device for grease_ACO: std" (IFCLABEL)
    Type Id = "ZZZ_do not use_ME_ST_measuring device for grease_ACO: std" (IFCLABEL)
    help_connected_phase = 1 (IFCINTEGER)
    option = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Circle Head - Project Datum" (IFCLABEL)
    Family and Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type Id = "Level: Circle Head - Project Datum" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "ME_PE_lipusmart p ob_ACO" (IFCTEXT)
  Other: 3 more contents on 0 objects not shown
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Circle Head - Project Datum" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
    RSen_C_code_article = "3553.36.00" (IFCTEXT)
    RSen_C_code_gtin = "4002626790583" (IFCTEXT)
    RSen_C_description = "ACO Fettabschd. LipuSmart-P-OB NS 3 Basisausführung oval Freiaufstellung PE" (IFCTEXT)
    RSen_C_type_comments = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "5" (IFCTEXT)
    RSen_C_code_article = "3300.11.22" (IFCTEXT)
    RSen_C_code_gtin = "04002626299253" (IFCTEXT)
    RSen_C_description = "ACO Fülleinheit für Eco-Jet-O,-OD,-R,-RD" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    Mark = "6" (IFCTEXT)
    RSen_C_code_article = "3300.11.50" (IFCTEXT)
    RSen_C_code_gtin = "04002626361080" (IFCTEXT)
    RSen_C_description = "ACO Fettschichtdickenmessung für Freiaufst. 3 m Kabel" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 0" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Grease separator plant as per DIN EN 1825 and DIN 4040-100" (IFCTEXT)
    LOD = "LOD 400" (IFCTEXT)
    Manufacturer = "ACO" (IFCTEXT)
    Model = "NS 3" (IFCTEXT)
    OmniClass Number = "23.70.50.00" (IFCTEXT)
    OmniClass Title = "Liquid Waste Handling Services" (IFCTEXT)
    Type Comments = "Building Supervisory Authority approval Z-54.1-414" (IFCTEXT)
    Type Name = "NS3" (IFCTEXT)
  Identity Data: 3 more contents on 0 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "NS3" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "std" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 4 objects (2 IFCBUILDINGELEMENTPROXY, 1 IFCDISTRIBUTIONCONTROLELEMENT, 1 IFCFLOWCONTROLLER)
    Manufacturer = "ACO" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    DN_sanitary = FALSE (IFCBOOLEAN)
    Host = "Level : Level 0" (IFCTEXT)
    Level = "Level: Level 0" (IFCLABEL)
    OD_sanitary = TRUE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    back = FALSE (IFCBOOLEAN)
    clearance_zone = FALSE (IFCBOOLEAN)
    filling_device = TRUE (IFCBOOLEAN)
    grease_measure_device = TRUE (IFCBOOLEAN)
    heating_rod = FALSE (IFCBOOLEAN)
    inlet_angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    left = FALSE (IFCBOOLEAN)
    outlet_DN100 = TRUE (IFCBOOLEAN)
    outlet_DN80 = FALSE (IFCBOOLEAN)
    right = TRUE (IFCBOOLEAN)
    sight_glass = FALSE (IFCBOOLEAN)
    vent_at_entry = TRUE (IFCBOOLEAN)
    vent_at_exit = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 0" (IFCTEXT)
    Level = "Level: Level 0" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device = TRUE (IFCBOOLEAN)
    grease_measure_device = TRUE (IFCBOOLEAN)
    heating_rod = FALSE (IFCBOOLEAN)
    inlet_angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    left = FALSE (IFCBOOLEAN)
    right = TRUE (IFCBOOLEAN)
    sight_glass = FALSE (IFCBOOLEAN)
    vent_at_entry = FALSE (IFCBOOLEAN)
    vent_at_exit = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Host = "Level : Level 0" (IFCTEXT)
    Level = "Level: Level 0" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1472.6 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    Host = "Level : Level 0" (IFCTEXT)
    Level = "Level: Level 0" (IFCLABEL)
    Offset = 1562.99999999999 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 type objects
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 19.0751742399957 (IFCAREAMEASURE) [SQUARE_METRE]
    B = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    D = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    DN = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    DN_vent = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    D_vent = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    FH = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    FW = 230. (IFCLENGTHMEASURE) [MILLI METRE]
    H1 = 1055. (IFCLENGTHMEASURE) [MILLI METRE]
    H2 = 985. (IFCLENGTHMEASURE) [MILLI METRE]
    H3 = 1680. (IFCLENGTHMEASURE) [MILLI METRE]
    H4 = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
    L1 = 1450. (IFCLENGTHMEASURE) [MILLI METRE]
    L2 = 1650. (IFCLENGTHMEASURE) [MILLI METRE]
    LF = 1410. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.408470746314892 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    W1 = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    W2 = 770. (IFCLENGTHMEASURE) [MILLI METRE]
    access_entry = 1 (IFCINTEGER)
    access_entry_X_position = 280. (IFCLENGTHMEASURE) [MILLI METRE]
    access_exit = 1 (IFCINTEGER)
    lipusmart_H = 1529. (IFCLENGTHMEASURE) [MILLI METRE]
    lipusmart_L = 660. (IFCLENGTHMEASURE) [MILLI METRE]
    lipusmart_W = 742. (IFCLENGTHMEASURE) [MILLI METRE]
    lipusmart_X = 725. (IFCLENGTHMEASURE) [MILLI METRE]
    lipusmart_pump_L = 757. (IFCLENGTHMEASURE) [MILLI METRE]
    vent_Z_position = 1336. (IFCLENGTHMEASURE) [MILLI METRE]
    vent_length = 315. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 14.3142269411421 (IFCAREAMEASURE) [SQUARE_METRE]
    B = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    D = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    DN = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    DN_vent = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    D_vent = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    FH = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    FW = 230. (IFCLENGTHMEASURE) [MILLI METRE]
    H1 = 1055. (IFCLENGTHMEASURE) [MILLI METRE]
    H2 = 985. (IFCLENGTHMEASURE) [MILLI METRE]
    H3 = 1680. (IFCLENGTHMEASURE) [MILLI METRE]
    H4 = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
    L1 = 1450. (IFCLENGTHMEASURE) [MILLI METRE]
    L2 = 1650. (IFCLENGTHMEASURE) [MILLI METRE]
    LF = 1410. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.76895530836454 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    W1 = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    W2 = 770. (IFCLENGTHMEASURE) [MILLI METRE]
    access_entry = 1 (IFCINTEGER)
    access_entry_X_position = 280. (IFCLENGTHMEASURE) [MILLI METRE]
    access_entry_diameter = 470. (IFCLENGTHMEASURE) [MILLI METRE]
    access_exit = 1 (IFCINTEGER)
    cover_Z_position = 1401. (IFCLENGTHMEASURE) [MILLI METRE]
    rib_height = 1352. (IFCLENGTHMEASURE) [MILLI METRE]
    rib_number = 4 (IFCINTEGER)
    rib_width = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    vent_Z_position = 1336. (IFCLENGTHMEASURE) [MILLI METRE]
    vent_length = 315. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.076167150313411 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00141803315444823 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    Area = 0.0889160362470397 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00155701384156889 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
    RSen_E_c01_apparent_power_phase_1 = 500. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_2 = 500. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_3 = 500. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
    RSen_E_c01_apparent_power_phase_1 = 12. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_2 = 0. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_3 = 0. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 2 type objects
    RSen_E_c01_load_classification = "Power" (IFCLABEL)
    RSen_E_powerfactor = 1. (IFCREAL)
  Electrical Engineering | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    RSen_E_c01_apparent_power = 1500. (IFCPOWERMEASURE) [WATT]
    RSen_E_connected_fase = 1 (IFCINTEGER)
  Electrical Engineering | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    RSen_E_c01_apparent_power = 12. (IFCPOWERMEASURE) [WATT]
    RSen_E_connected_fase = 1 (IFCINTEGER)
  Electrical Engineering | properties | on 1 type object
    RSen_E_c01_3_phase = TRUE (IFCBOOLEAN)
    RSen_E_c01_current = 16. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c01_number_of_poles = 3 (IFCINTEGER)
    RSen_E_c01_subclass_motor = TRUE (IFCBOOLEAN)
    RSen_E_c01_voltage = 400. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Electrical Engineering | properties | on 1 type object
    RSen_E_c01_3_phase = FALSE (IFCBOOLEAN)
    RSen_E_c01_current = 0.05 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c01_number_of_poles = 1 (IFCINTEGER)
    RSen_E_c01_subclass_motor = FALSE (IFCBOOLEAN)
    RSen_E_c01_voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    RSen_P_c01_diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c03_diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c04_diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c06_diameter = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    RSen_C_intended_use = "Entwässerungssysteme" (IFCTEXT)
  General | properties | on 1 type object
    RSen_C_code_ETIM = "EC010271" (IFCTEXT)
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_code_specification_URL = "https://de.bim.aco/haustechnik/text_35533600_ACO-HT_de.txt" (IFCTEXT)
    RSen_C_content_creator = "Itannex bv" (IFCTEXT)
    RSen_C_content_date_changed = "" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "" (IFCTEXT)
    RSen_C_info_technical = "https://de.bim.aco/haustechnik/datasheet_3553.36.00_ACO-HT_de.pdf" (IFCTEXT)
    RSen_C_intended_use = "Entwässerungssysteme" (IFCTEXT)
    installation_manual = "" (IFCTEXT)
    instructions_for_use = "" (IFCTEXT)
  General | properties | on 1 type object
    RSen_C_code_ETIM = "EC010071" (IFCTEXT)
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_code_specification_URL = "" (IFCTEXT)
    RSen_C_content_creator = "Itannex bv" (IFCTEXT)
    RSen_C_content_date_changed = "" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "" (IFCTEXT)
    RSen_C_info_technical = "" (IFCTEXT)
    RSen_P_c01_diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    installation_manual = "" (IFCTEXT)
    instructions_for_use = "" (IFCTEXT)
  General | properties | on 1 type object
    RSen_C_code_ETIM = "-" (IFCTEXT)
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_code_specification_URL = "" (IFCTEXT)
    RSen_C_content_creator = "Itannex bv" (IFCTEXT)
    RSen_C_content_date_changed = "" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "" (IFCTEXT)
    RSen_C_info_technical = "" (IFCTEXT)
    installation_manual = "" (IFCTEXT)
    instructions_for_use = "http://catalogue.aco-buildingdrainage.com/ilcatalogue/download/ZG9jdW1lbnQvZG93bmxvYWQucGRmL2RlL2ViYV8xMC4wMi4xMF9kZV8zMzAwLjExLjUwX2tsX18xMzg4MTIucGRm/eba_10.02.10_de_3300.11.50_kl__138812.pdf" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    RSen_P_c04_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Classification = "Sanitary,Vent,Domestic Cold Water,Power,Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    System Classification = "Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Model Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    clearance_back = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    clearance_entry = 1825. (IFCLENGTHMEASURE) [MILLI METRE]
    clearance_exit = 1385. (IFCLENGTHMEASURE) [MILLI METRE]
    clearance_front = 1178. (IFCLENGTHMEASURE) [MILLI METRE]
    clearance_top = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
  Model Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    filling_device_CL = 272.6 (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_X = 1081. (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_Y = 470.8 (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_Z = 973.6 (IFCLENGTHMEASURE) [MILLI METRE]
    filling_device_position = 135. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    glass_X = 1017.5 (IFCLENGTHMEASURE) [MILLI METRE]
    glass_Z = 930.5 (IFCLENGTHMEASURE) [MILLI METRE]
    glass_position = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    grease_measure_X = 530. (IFCLENGTHMEASURE) [MILLI METRE]
    grease_measure_Y = 550. (IFCLENGTHMEASURE) [MILLI METRE]
    grease_measure_Z = 1352. (IFCLENGTHMEASURE) [MILLI METRE]
    grease_measure_end_angle = 265. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    grease_measure_position = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    grease_measure_start_angle = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    heatrod_X = 705. (IFCLENGTHMEASURE) [MILLI METRE]
    heatrod_Z = 690. (IFCLENGTHMEASURE) [MILLI METRE]
    heatrod_position = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    waterinlet_end_angle = 50. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    waterinlet_start_angle = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Phasing | properties | on 4 objects (2 IFCBUILDINGELEMENTPROXY, 1 IFCDISTRIBUTIONCONTROLELEMENT, 1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Plumbing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    grease_store_capacity = 0.15 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    overall_capacity = 0.63 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    pump_tank_capacity = 0.295 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    sludge_trap_capacity = 0.3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    usable_pump_tank_capacity = 0.155 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Plumbing | properties | on 1 type object
    p_c01_flow = 0.003 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Structural | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    RSen_S_gross_mass = 833.6 (IFCREAL)
    RSen_S_net_mass = 203.6 (IFCREAL)
  Structural | properties | on 1 type object
    RSen_S_net_mass = 3.5 (IFCREAL)
  Structural | properties | on 1 type object
    RSen_S_net_mass = 2.8 (IFCREAL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Anno_Level_Head_Circle: Standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = FALSE (IFCBOOLEAN)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "std" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 2 type objects
    RSen_C_material = "HDPE, Grey" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "Stainless Steel, Brushed" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "HDPE, Black" (IFCLABEL)